|  |
| --- |
| Technical Data |
|

|  |
| --- |
|  |

|  |  |
| --- | --- |
| Model Name  | MVR500-1000VA  |
| Product Type  | Automatic voltage regulator  |
| Capacity  | 500 VA / 300 W    1000VA/600W  |
| Input  |
|  Voltage   | 220+-%25VAC  |
|  Voltage Range  | 176 ~ 272VAC  |
|  Frequency  | 50Hz/60HZ  |
| AVR  |
|  Output  | Adjustable 220v  |
| LED  |
|  Power on / off  | Green LED  |
|  AVR LED  | Boost: red LED; buck: red LED  |
| Environment  |
|  Operating Temperature  | 0° - 40 ° C at full load  |
|  Humidity   | Relative, 0% ~ 90% (non condensing)  |
|  Noise Level   | Less than 40dB  |
| Interface  |
|  Electrical Outputs  | SCHUKO \* 4 / NEMA \* 6  |
|  Telephone/Modem Jack  | Yes  |
|  Interface  | N/A  |
| Measurements  |
|  Dimensions (D x W x H)  | 192 x 115 x 113 mm  |
|  Net Weight  | 1.8/2.3 kgs  |

 |