|  |
| --- |
| Technical Data |
| |  | | --- | |  |  |  |  | | --- | --- | | Model Name | MVR500-1000VA | | Product Type | Automatic voltage regulator | | Capacity | 500 VA / 300 W    1000VA/600W | | Input | | | Voltage | 220+-%25VAC | | Voltage Range | 176 ~ 272VAC | | Frequency | 50Hz/60HZ | | AVR | | | Output | Adjustable 220v | | LED | | | Power on / off | Green LED | | AVR LED | Boost: red LED; buck: red LED | | Environment | | | Operating Temperature | 0° - 40 ° C at full load | | Humidity | Relative, 0% ~ 90% (non condensing) | | Noise Level | Less than 40dB | | Interface | | | Electrical Outputs | SCHUKO \* 4 / NEMA \* 6 | | Telephone/Modem Jack | Yes | | Interface | N/A | | Measurements | | | Dimensions (D x W x H) | 192 x 115 x 113 mm | | Net Weight | 1.8/2.3 kgs | |